nRF\_DFU

components\ble\ble\_services\ble\_dfu\ble\_dfu.c

components\ble\ble\_services\ble\_dfu\ble\_dfu\_bonded.c

components\ble\ble\_services\ble\_dfu\ble\_dfu\_unbonded.c

nRF\_BLE

components\ble\peer\_manager\gatt\_cache\_manager.c

components\ble\peer\_manager\gatts\_cache\_manager.c

components\ble\peer\_manager\id\_manager.c

components\ble\peer\_manager\peer\_data\_storage.c

components\ble\peer\_manager\peer\_database.c

components\ble\peer\_manager\peer\_id.c

components\ble\peer\_manager\peer\_manager.c

components\ble\peer\_manager\peer\_manager\_handle.c

components\ble\peer\_manager\pm\_buffer.c

components\ble\peer\_manager\security\_dispatcher.c

components\ble\peer\_manager\security\_manager.c

nRF\_Libraries

components\libraries\fds\fds.c

components\libraries\crc16\crc16.c

components\libraries\fstorage\nrf\_fstorage.c

components\libraries\fstorage\nrf\_fstorage\_sd.c

nRF\_svc

components\libraries\bootloader\dfu\nrf\_dfu\_svci.c

nrfutil pkg generate --hw-version 52 --application-version 1 --application Impedance\_no\_switch\_test1.hex --sd-req 0xaf --key-file private.key Impedance\_no\_switch\_test1.zip